Rover VVC
EU2

36-way ECU connector


	Pin number
	Normal use
	VVC Emerald ECU

	1
	Injector driver 4
	Injector 2

	2
	IACV
	Channel 2

	3
	IACV
	Channel 1

	4
	Main relay control
	Main relay control

	5
	Ignition driver 2
	Coil 2

	6
	Cooling fan relay control
	Cooling fan relay

	7
	Oxygen sensor 1 signal input
	0-1v (narrow band) input

	8
	Throttle pot signal input
	0-5v input

	9
	Throttle pot supply / +5v out
	TPS / MAP +5v supply

	10
	AuxIn10
	Oil temp sensor signal

	11
	Ignition sense input
	+12v supply via ignition switch

	12
	Tacho output signal
	12v pulsed output

	13
	Immobilisor input
	Immobilisor signal / Aux digital input

	14
	+8v out
	Not used

	15
	Cam phase
	Cam sensor signal

	16
	Air temperature signal input
	ATS

	17
	AuxOut17
	VVC increase

	18
	Oxygen sensor signal earth
	Lambda signal earth

	19
	Shift-light driver
	

	20
	Fuel pump relay driver
	Fuel pump driver

	21
	AuxOut21
	VVC decrease

	22
	IACV
	Channel 3

	23
	Injector driver 2
	Injector 3

	24
	Injector driver 1
	Injector 1

	25
	Ignition driver 1
	Coil 1

	26
	Injector driver 3
	Injector 4

	27
	IACV
	Channel 4

	28
	+12v Ignition supply
	+12v supply

	29
	ECU earth
	System earth

	30
	Sensor earth (common earth)
	Common sensor earth

	31
	Main trigger signal input
	Crank sensor signal

	32
	Main trigger sensor earth
	Crank / Cam sensor earth

	33
	Coolant temp signal input
	CTS

	34
	AuxIn34
	MAP signal

	35
	AuxIn35
	

	36
	AuxIn36 / AuxOut36
	AuxOut36 - Lambda heater relay control


VVC loom RED connector

	Pin Number
	Wire colour
	Function
	Emerald K3 plug

	1
	Red/yellow
	Cam sensor +
	15

	2
	Black/blue
	Cam sensor -
	32

(join with wire from Red26)

	3
	
	
	

	4
	
	
	

	5
	
	
	

	6
	
	
	

	7
	
	
	

	8
	
	
	

	9
	Black/white
	Tacho output
	12

	10
	Orange/green
	IACV
	22

	11
	
	
	

	12
	Yellow/brown
	Injector, cylinder 1
	24

	13
	Yellow/red
	Injector, cylinder 2
	1

	14
	Yellow/white
	Injector, cylinder 3
	23

	15
	Orange/blue
	IACV
	27

	16
	
	
	

	17
	Yellow/orange
	-
	-

	18
	
	
	

	19
	
	
	

	20
	
	
	

	21
	
	
	

	22
	
	
	

	23
	Black
	Crank/Cam cable shield
	32

(join with wire from Red2)

	24
	
	
	

	25
	Blue/purple
	Crank sensor +
	31

	26
	Blue/white
	Crank sensor -
	32

(join with wire from Red2)

	27
	Grey
	Lambda sensor signal
	7

	28
	Green/grey
	Lambda sensor earth
	18

	29
	
	
	

	30
	
	
	

	31
	
	diagnostics
	-

	32
	Brown/Black
	Engine bay cooling fan relay
	-

	33
	Pink/blue
	IACV
	2

	34
	Orange/grey
	IACV
	3

	35
	Yellow/black
	Injector, cylinder 4
	26

	36
	
	
	


VVC loom BLACK connector
	Pin Number
	Wire colour
	Function
	Emerald K3 plug

	1
	
	
	

	2
	Brown/black
	VVC increase
	17

	3
	
	
	

	4
	
	
	

	5
	
	
	

	6
	
	
	

	7
	
	
	

	8
	Red/green?
	+5v sensor supply (MAP sensor)
	9

(join with wire from Black18)

	9
	
	
	

	10
	Green/orange
	Oil temp sensor signal
	10

	11
	Grey/white
	Engine bay temp signal
	-

	12
	Yellow/green
	Throttle pot signal
	8

	13
	Pink/black
	Sensor earth
	30

	14
	Black/green
	Air temp sensor signal
	16

	15
	Pink/green
	Coolant temp sensor signal
	33

	16
	-
	-
	-

	17
	Yellow/red
	Immobiliser input
	13

	18
	Yellow/purple
	+5v sensor supply (TPS)
	9

(join with wire from Black8)

	19
	-
	-
	-

	20
	Black/green
	Oxygen sensor heater relay
	36

	21
	Black
	ECU earth
	29

	22
	White/pink
	Main relay control
	4

	23
	Black/yellow
	VVC decrease
	21

	24
	-
	-
	-

	25
	White/black
	Ignition coil 1
	25

	26
	White/black
	Ignition coil 2
	5

	27
	Brown/pink
	+12v from main relay
	28

	28
	Blue/grey
	Cooling fan relay
	6

	29
	-
	-
	-

	30
	Black/purple
	Fuel pump relay
	20

	31
	Green/brown
	-
	-

	32
	-
	-
	-

	33
	White
	Ignition sense
	11

	34
	
	
	

	35
	
	
	

	36
	Yellow/purple
	MAP sensor signal
	34
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Rear view of connector








