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Parameter (Click + to select)

Live data update interval 647ms
Engine speed 0 RPM
Stepper motor position 140 steps
Throttle position sensor 09V

Coil charge time 72ms
Ignition switch On

Purge duty cycle 0%

Idle error 31568 rpm
Loop status Open loop
Battery voltage 1.0V

Air / fuel ratio 1461
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Parameter (Click + to select)
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Parameter (Click + to select)

Live data update interval 649ms
Trinary switch ?

Throttle position sensor 09V

Air / fuel ratio 1461
Oxygen sensor voltage 044V
Oxygen sensor frequency Invalid value
Oxygen sensor duty cycle Invalid value
Oxygen sensor status Okay

Coil charge time 72ms
Park/Neutral switch Open

Idle switch Closed

Air con switch Open

Idle set point 0 RPM

Idle deadband (HotDB Pos) 35 steps
Stepper motor position 140 steps
Idle speed deviation 1200 rpm
Ignition advance offset 0.0°
Ignition advance 50°
Coolant temperature 17°C
Ignition switch On

Throttle angle 125°
Ambient air temperature Invalid value
Intake air temperature 35°C

Fuel rail temperature Invalid value
Inlet manifold pressure 95 kPa
Battery voltage 1.0V
Loop status Open loop
Shart term trim / Feadhack 100 °%
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- |Short term trim / Feedback

- |Long term trim / Inj dead time 0uS

- |Purge duty cycle 0%

- |ldle error 31568 rpm

- |Idle runline position 255 steps

- |Jack count 1 steps

- |Engine speed 0RPM
- [Crank status Synced





